SERV MANUAL UPDATE-SEC.7A ENGINE TO TRANS TORQUE SPEC. Pontiac Sunbird 1990

For 1990-2009 cars

# SERV MANUAL UPDATE-SEC.7A ENGINE TO TRANS TORQUE SPEC

#### Subject: SERVICE MANUAL UPDATE-SECTION 7A-AUTOMATIC TRANSAXLE-ENGINE TO TRANS TORQUE SPECIFICATIONS Models Affected: 1989-1991 SUNBIRD MODELS WITH 3T40

An error exists in the engine to transaxle mounting illustrations. The specification shows 75 N.m (85 lbs. ft.) . The correct specification for the stud or bolt is 75 N.m (55 lbs. ft.).

This information applies to the following manuals.

YEAR MODEL PAGE FIGURE ---- ----- ---- ------ 1989 Sunbird 7A-25 44

1990 Sunbird 7A-26 44

1991 Sunbird 7A-27 and 7A-28 47 and 48

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.