FRONT STABILIZER BAR INSULATOR BUSHING SQUEAK. Pontiac Sunbird 1984

For 1990-2009 cars

# FRONT STABILIZER BAR INSULATOR BUSHING SQUEAK

A squawk noise from the front stabilizer bar insulator bushings may be corrected by installing new Teflon lined bushings. The new bushings are being used in production beginning approximately February 1, 1986.

Bushing part numbers and applications are shown below:

Stabilizer Bar Bushing 24mm Shaft Diameter

Part Number 22532210 1986 Sunbird (except F41, WS6) (Replaces No. 14085145) 1984 Sunbird (1.8L, 2.0L, except Y99) 1985 Sunbird (1.8L, 2.0L, except F41) 1985-86 Grand Am (2.5L, except F41)

Stabilizer Bar Bushing 26mm Shaft Diameter

Part Number 22532211 1985-86 Grand Am (3.0L, except FE2, (Replaces No. 14085146) FE3, F41)

Stabilizer Bar Bushing 28mm Shaft Diameter

Part Number 22532212 1984 Sunbird (with Y99) (Replaces No. 14085147) 1985-86 Sunbird (with F41, WS6) 1985 Grand Am (with F41) 1986 Grand Am (3.0L, except F41)

Stabilizer Bar Bushing 30mm Shaft Diameter

Part Number 22532213 1986 Grand Am (with F41) (Replaces No. 14085148)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.