THROTTLE BODY INSTALLATION REVISED TORQUE SPECIFICATIONS. Pontiac Sunbird 1985

For 1990-2009 cars

# THROTTLE BODY INSTALLATION REVISED TORQUE SPECIFICATIONS

#### VEHICLES AFFECTED: 1985 Cavaller Models Equipped with 2.0L L-4 Engine

The installation torque of the three throttle body attaching bolts has been changed to 23 Nm (17 ft. lbs). Step 6, TBI Installation Procedure, on page 6E2-76 of the 1985 Cavalier Shop Manuals (ST-366-85 and ST-388-85) should be revised to show this information.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.