CREAK CONDITION, FRT. SEATS INSTALL NEW SPACER. Pontiac Sunbird 1992

For 1990-2009 cars

# CREAK CONDITION, FRT. SEATS INSTALL NEW SPACER

#### SUBJECT: BUCKET FRONT SEAT CREAK CONDITION DUE TO SPACE BETWEEN PIVOT PIN AND BUSHING (INSTALL SPACER)

#### MODELS AFFECTED: 1992 GRAND AM AND SUNBIRD MODELS W/AR9 OPTION

THIS BULLETIN IS BEING REVISED TO CHANGE THE CAUSE AND CORRECTION SECTIONS. THIS BULLETIN CANCELS AND REPLACES BULLETIN 92-10-42A. PLEASE DISCARD BULLETIN 92-10-42A.

APPLICATION: All 1992 Grand Am and Sunbird series vehicles with front bucket (AR9) seats.

CONDITION: Some owners of 1992 Grand Am and Sunbird models with AR9 bucket front seats may comment that when making a sharp right or left turn, a creaking noise from the driver seat, and front passenger seat (when occupied) occurs.

CAUSE: Excessive space between the inner front seatback pivot pin and the pivot bushing.

#### CORRECTION:

1. Put seatback in its most forward position.

2. From rear of seat, install spacer GM P/N 16743252 on pivot pin.

#### PART AVAILABILITY:

Parts are currently available from GMSPO.

LABOR OPERATION: T1818

LABOR TIME 0.2 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.