CAMPAIGN: REAR LAMP WIRING HARNESS. Pontiac Sunbird 1988

For 1990-2009 cars

# CAMPAIGN: REAR LAMP WIRING HARNESS

#### Models: 1988 Cavalier & Sunbird Coupes & Convertibles (37 and 67)

#### TO: ALL GENERAL MOTORS DEALERS

#### CONDITION:

--------- General Motors of Canada has determined that some 1988 Cavalier and Sunbird Coupes and Convertibles fail to conform to the requirements of Federal Motor Vehicle Safety Standard 108, "Lamps, Reflective Devices, and Associated Equipment." The above referenced vehicles may have been assembled with rear lamp wiring harnesses that contain open or intermittent circuits affecting back-up lamp or license plate lamp operation. This condition may cause these lamps to flash or be inoperative. To prevent this condition from occurring, the rear lamp wiring harness will be replaced on all involved vehicles.

#### VEHICLES INVOLVED:

Certain 1988 Cavalier and Sunbird 37 and 67 style models within the following VIN breakpoints: Up To And Series Assembly Plant Beginning Including ------ -------------- --------- --------- Cavalier JC, JE, JF Janesville S.O.P. JJ121878

Cavalier JC, JE, JF Lordstown S.O.P. J711OZ41

Sunbird JD, JU Lordstown S.O.P. J7506772

All affected vehicles have been identified by the VIN listing provided to involved Dealers with this bulletin. Any Dealer not receiving a listing was not shipped any of the affected vehicles.

#### DEALER CAMPAIGN RESPONSIBILITY:

Dealers are to service all vehicles subject to this campaign at no charge to owners, regardless of mileage, age of vehicle, or ownership, from this time forward.

Whenever a vehicle subject to this campaign is taken into your new or used vehicle inventory, or it is in your Dealership for service in the future, you should take the steps necessary to be sure the campaign correction has been made before reselling or releasing the vehicle.

Owners of vehicles recently sold from your new vehicle inventory are to be contacted by the Dealer, and arrangements made to make the required modification according to instructions contained in this bulletin.

#### CAMPAIGN PROCEDURE:

Refer to Section 4 of the Service Policies and Procedures Manual for the detailed procedure on handling Product Campaigns. Dealers are requested to complete the campaign on all transfers as soon as possible.

#### OWNER NOTIFICATION:

All owners of record at the time of campaign release are shown on the attached computer listing and have been notified by first class mail from General Motors. The listings provided are for campaign activity only and should not be used for any other purpose.

#### PARTS INFORMATION:

Parts required should be ordered through regular channels, as follows:

Quantity Description Part Number Per Vehicle ----------- ----------- ----------- Harness - Body Rear & Compartment Lid 12083281 1 Jumper Wiring (Without Deck Lid Carrier)

Harness - Body Rear & Compartment Lid 12083282 1 Jumper Wiring (with Deck Lid Carrier, V56; and/or Convertible Body Style)

#### PARTS AND LABOUR CLAIM INFORMATION:

Credit for the campaign work performed will be paid upon receipt of a properly completed campaign claim card, RAPID terminal or DCS transmission in accordance with the following:

Repair Code Description Time Allowance ----------- ----------- -------------- 2A Replace Rear Lamp Wiring Harness .4

Time allowance includes 0.1 hour for Dealer administrative detail associated with this campaign. Parts credit will be based on Dealer net plus 30% to cover parts handling.

#### SERVICE PROCEDURE:

(CHEVROLET) VEHICLES WITH DECK LID CARRIER OR CENTER HIGH MOUNTED STOP LAMP ON THE DECK LID:

1. Raise deck lid and disconnect the four-wire connector just ahead of the left deck lid hinge (outboard of radio speaker). Driver's side of vehicle is left.

2. On underside of deck lid, across rear, unclip the three male/female connectors from the sheet metal edges of three holes. In the hole which has the rear compartment lamp, also remove the harness clip. All four clips are silver colored. Break the two connections to the back-up/licence plate lamp jumpers and the connection to the center high mounted stop lamp (CHMSL) jumper.

3. Remove the harness from the clips on the left hinge and fish it out through the hole in the deck lid at the left reflectors (outboard of left backup lamp).

A piece of string tied to the harness being removes will speed installation of the replacement harness up through the deck lid.

4. Install new harness (part number 12083282) in deck lid.

5. Reconnect all connections, snap all four silver clips onto sheet metal edges, and place harness in clips on hinge.

6. Check for proper operation of center high mounted stop lamp, back-up, and license lamps.

7. Install Campaign Identification Label.

#### (CHEVROLET) J37 VEHICLE WITHOUT DECK LID CARRIER:

1. Raise deck lid and disconnect the four-wire connector just ahead of the left deck lid hinge (outboard of radio speaker). Driver's side of vehicle is left.

2. On underside of deck lid, across rear, unclip the two male/female connectors from the sheet metal edges of two holes. In the hose which has the rear compartment lamp, also remove the harness clip. All three clips are silver colored. Break the two connections to the back-up/licence plate lamp jumpers.

3. Enter passenger compartment; pull cover off of center high mounted stop lamp on the trim panel behind the rear seat (it is held on with velcro). Disconnect wires and push through the hole in the shelf.

4. Return to rear compartment. Remove the harness from the clips on the left hinge and fish it out through the hole in the deck lid at the left reflectors (outboard of left back-up lamp).

A piece of string tied to the harness being removed will speed installation of the replacement harness up through the deck lid.

5. Install new harness (part number 12083281) in deck lid. Reconnect all connections, snap all three silver clips onto sheet metal edges, and place harness in clips on hinge.

6. Push wire up into center high mounted stop lamp housing. Enter passenger compartment, reconnect wires, and reinstall cover. Return to rear compartment.

7. Check for proper operation of center high mounted stop lamp, back-up, and license lamps.

8. Install Campaign Identification Label.

(PONTIAC) VEHICLES WITH DECK LID CARRIER OR CENTER HIGH MOUNTED STOP LAMP MOUNTED ON THE DECK LID: ----------------------------------------------------------------------------- 1. Raise deck lid and disconnect the four-wire connector just ahead of the left deck lid hinge (outboard of radio speaker). Driver's side of vehicle is left.

2. On underside of deck lid, across rear, unclip the three male/female connectors from the sheet metal edges of three holes. In the hole which has the trunk light, also remove the harness clip. All four clips are silver colored. Break the two connections to the back-up lamp jumpers and the connection to the center high mounted stop lamp (CHMSL) jumper.

3. Remove the harness from the clips on the left hinge and fish it out through the hole in the deck lid at the left reflectors (outboard of left backup lamp).

A piece of string tied to the harness being removed will speed installation of the replacement harness up through the deck lid.

4. Install new harness (part number 12083282) in deck lid.

5. Reconnect all connections, snap all four silver clips onto sheet metal edges, and place harness in clips on hinge.

6. Check for proper operation of center high mounted stop lamp, and back-up lamp.

7. Install Campaign Identification Label.

#### (PONTIAC) J37 VEHICLES WITHOUT LID CARRIER:

1. Raise deck lid and disconnect the four-wire connector just ahead of the left deck lid hinge (outboard of radio speaker). Driver's side of vehicle is left.

2. On underside of deck lid, across rear, unclip the two male/female connectors from the sheet metal edges of two holes. In the hole which has the trunk light, also remove the harness clip. All three clips are silver colored. Break the two connections to the back-up lamp jumpers.

3. Enter passenger compartment; pull cover off the center high mounted stop lamp on the trim panel behind the rear seat (it is held on with velcro). Disconnect wires and push through the hole in the shelf.

4. Return to rear compartment. Remove the harness from the clips on the left hinge and fish it out through the hole in the deck lid at the left reflectors (outboard of left back-up lamp).

A piece of string tied to the harness being removed will speed installation of the replacement harness up through the deck lid.

5. Install new harness (part number 12083281) in deck lid. Reconnect all connections, snap all three silver clips onto sheet metal edges, and place harness in clips on hinge.

6. Push wire up into center high mounted stop lamp housing. Enter passenger compartment, reconnect wires, and reinstall cover. Return to rear compartment.

7. Check for proper operation of center high mounted stop lamp and back-up lamp.

8. Install Campaign Identification Label.

#### INSTALLATION OF CAMPAIGN IDENTIFICATION LABEL

Clean surface of radiator upper mounting panel and apply a Campaign Identification Label. Make sure the correct campaign number is inserted on the label. This will indicate that the campaign has been completed.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.