CONV. BOOT DIFFICULT TO ATTACH RUBBER RETAINER TO MOLDING. Pontiac Sunbird 1989

For 1990-2009 cars

# CONV. BOOT DIFFICULT TO ATTACH RUBBER RETAINER TO MOLDING

#### SUBJECT: CONVERTIBLE BOOT DIFFICULT TO ATTACH RUBBER RETAINER TO MOULDING (DIAGNOSIS AND REPAIR)

#### VEHICLES AFFECTED: 1988-89 J CAR CONVERTIBLE

Some owners of 1988 and 1989 Pontiac and/or Chevrolet J body convertibles may comment on the boot not retaining to the moulding after installation at the rear outboard corners.

#### Inspect:

------- 1. Lower the convertible top and install the top boot as described in the Convertible Owners Manual Supplement.

2. Check the retention of the boot rubber retainer to the moulding at the rear outboard corners. If the retention of the boot retainer to the moulding is unsatisfactory, or if rubber retainer does not retain to the moulding, the boot rubber retainer may be modified as follows:

#### Top Boot

Remove or Disconnect (See Figure 1)

1. Top boot from moulding.

2. Using a sharp knife, cut lower lip of boot rubber retainer as shown in illustration.

#### Install or Connect

1. Top boot to moulding.

#### Inspect

Top boot rubber retainer for proper retention to moulding.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.