WINDSHIELD WASHER FLUID LOSS (REPL. WINDSHIELD WASHER) RESE. Pontiac Sunbird 1993

For 1990-2009 cars

# WINDSHIELD WASHER FLUID LOSS (REPL. WINDSHIELD WASHER) RESE

#### SUBJECT: WINDSHIELD WASHER FLUID LOSS (REPLACE WINDSHIELD WASHER RESERVOIR AND BRACKET)

#### VEHICLES AFFECTED: 1992-93 "J" SERIES

#### CONDITION:

--------- Some 1992-93 "J" vehicles may experience windshield washer fluid loss with cracked reservoirs.

#### CAUSE:

----- This may be caused by abrasion from the reservoir bracket edge.

#### CORRECTION:

---------- Replace affected washer reservoir and replace bracket with a revised nylon coated bracket, P/N 22593352.

1. Remove washer bottle filler neck bolt and cap assembly.

2. Remove front air induction tube bolt.

3. Remove battery. Refer to service manual, section 6D1.

4. Remove washer reservoir bracket bolts in battery tray.

5. Raise vehicle and suitably support. Refer to service manual, section OB.

6. Remove left front wheel. Refer to service manual, section 3E.

7. Remove front inner fender bolts and move aside.

8. Remove left front valance bolts and clips.

9. Disconnect washer pump and electrical connection.

10. Remove lower washer reservoir bracket bolt through hole in valance.

11. Remove lower air induction tube.

12. Remove washer reservoir.

13. Transfer washer pump to new bottle.

14. Remove bracket.

15. Install revised bracket.

16. Install washer reservoir.

17. Install air induction tube and lower bolt.

18. Install lower reservoir bracket bolt through hole in valance.

19. Install washer pump hose and electrical connector.

20. Install front valance bolts and clips on left side.

21. Install inner fender assembly.

22. Install wheel. Refer to service manual, section 3E.

23. Lower vehicle.

24. Install front air induction tube bolt.

25. Install washer bottle bracket bolts in battery tray.

26. Install washer reservoir filler neck bolt and cap.

27. Install battery. Refer to service manual, section 6D1.

28. Refill reservoir and check washer system for proper operation.

For vehicles repaired under warranty use:

Labour Operation: N3750 Labour Time: .9

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.