UNIBODY COLLISION REPAIR AND WELDED PANEL REPLACEMENT. Pontiac Sunbird 1989

For 1990-2009 cars

# UNIBODY COLLISION REPAIR AND WELDED PANEL REPLACEMENT

TWO NEW SECTIONS HAVE BEEN ADDED TO ALL GENERAL MOTORS J AND N CARLINE SERVICE MANUALS. THESE SECTIONS ARE:

11-1 UNIBODY COLLISION REPAIR 11-2 WELDED PANEL REPLACEMENT

THESE SECTIONS PROVIDE INFORMATION ON THE PROPER PROCEDURE TO USE WHEN PERFORMING COLLISION OR WELDED PANEL REPLACEMENT. SECTION 11-2 CAN ALSO BE USED TO IDENTIFY THE LOCATION AND APPLICATION OF WELDS AND SEALERS WHEN DIAGNOSING UNUSUAL WATER LEAK OR SQUEAK CONCERNS.

AFTER YOU HAVE HAD A CHANCE TO REVIEW THESE NEW SECTIONS, WE WOULD LIKE YOUR FEEDBACK. DO YOU FIND THE INFORMATION:

- USEFUL - UNDERSTANDABLE - COMPLETE

ANY OTHER COMMENTS ON THESE NEW SECTIONS WOULD ALSO BE APPRECIATED. SEND YOUR COMMENTS TO:

OLDSMOBILE DIVISION PRODUCT SERVICE ENGINEERING ATTENTION: PUBLICATIONS 920 TOWNSEND LANSING, MI. 48921-7042

(OTHER DIVISIONS, PLEASE USE YOUR ADDRESS BUT PLEASE SEND COMMENTS TO OLDSMOBILE DIVISION.)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.