SERVICE MAN. UPDATE SEC.7A ENGINE TO TRANS TORQUE SPECS. Pontiac Sunbird 1989

For 1990-2009 cars

# SERVICE MAN. UPDATE SEC.7A ENGINE TO TRANS TORQUE SPECS

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 7A-AUTOMATIC TRANSAXLE ENGINE TO TRANS TORQUE SPECIFICATION

#### VEHICLES AFFECTED: 1989 - 1991 'J' MODELS WITH, 3T40

An error exists in the engine to transaxle mounting illustrations. The specification shows 75 N.m (85 ft.lbs.). The correct specification for the stud or bolt is 75 N.m (55 ft.lbs.)

YEAR MODEL PAGE FIGURE ---- -------- ----- ------ 1989 Buick Skyhawk 7A-24 41 1989 Chevrolet Cavalier 7A-25 46 and 47 1989 Pontiac Sunbird 7A-25 44

1990 Chevrolet Cavalier 7A-27 46 and 47 1990 Pontiac Sunbird 7A-26 44

1991 Chevrolet Cavalier 7A-27 and 7A-28 47 and 48 1991 Pontiac Sunbird 7A-27 and 7A-28 47 and 48

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.