LABOR OPERATION D3000 A/C SYS. LEAK TEST PARTIAL CHARGE. Pontiac T1000 1984

For 1990-2009 cars

# LABOR OPERATION D3000 A/C SYS. LEAK TEST PARTIAL CHARGE

LABOR OPERATION D3000 "A/C SYSTEM - LEAK TEST AND PARTIAL CHARGE " SHOULD BE USED TO PARTIALLY CHARGE A COMPLETELY DISCHARGED SYSTEM TO LOCATE A LEAK DUE TO A COMPONENT FAILURE. IT IS NOT NECESSARY TO FULLY CHARGE THE SYSTEM TO PERFORM SUCCESSFUL LEAK TESTING. EFFECTIVE IMMEDIATELY: THIS LABOR OPERATION TO BE USED TO PARTIALLY CHARGE (1 LB. MAX.) THE A/C SYSTEM TO LOCATE A LEAK. "OTHER LABOR HOURS" NOT ALLOWED WITH THIS LABOR OPERATION; NECESSARY REPAIRS OR COMPONENT REPLACEMENT MUST BE CLAIMED WITH APPROPRIATE LABOR OPERATION.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.