LTG REQUEST FOR REVIEW MARCH -aprIL. Pontiac T1000 1987

For 1990-2009 cars

# LTG REQUEST FOR REVIEW MARCH -aprIL

This bulletin addresses changes to the published Pontiac Labor Time Guide; March and April changes are attached. These changes are the result of dealer "Requests For Review" being handled by C-P-C Technical Service Activity.

These updates will be included in future 1987 Labor Time Guide revisions. In the case of past model year updates, it is recommended that this bulletin be retained with all appropriate model year Labor Time Guides, as a complete revision will not be provided.

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G J T H N P NUMBER VIN CODE --------- -------

SPOILER - R&R OR REPLACE Applicable model years: 1986-1987 ONE PIECE B5608 .3 .3 ADD: A-To Transfer High Level Stop Lamp .1 .1

CREST, EMBLEM OR COVER, REAR COMPARTMENT LID LOCK CYLINDER-REPLACE B8610 .3 NOTE: Applicable model year 1987

GLASS, BACK WINDOW C0660 2.0 -REPLACE NOTE: Applicable model team 1986-1987 ADD: A-W/Rear Spoiler .3

HEADLINING ASSEMBLY-REPLACE NOTE: Applicable model team: All. '35' styles only. FRONT C3122 1.4 REAR C3123 .9 COMPLETE C3127 2.0

PLATE, FRONT DOOR ARMREST SWITCH MOUNTING-R&R OR REPLACE NOTE: Applicable model team: 1986-1987 RIGHT C3300 .2 LEFT C3301 .2

MOTOR AND/OR FAN, BLOWER - R&R OR REPLACE HEATER D1320 V-6 .7 A/C D1322 NOTE: Applicable model year 1987 V-6 .7 LEVER, MULTIFUNCTION E7060 - REPLACE NOTE: Applicable model yeam: 1985-1987 ADD: A-To Color Coat .1 GB

GEAR ASSEMBLY, POWER E9730 STEERING SHORT - REPLACE NOTE:Applicable model years: 1985-1987 ADD: A- W/Locking Wheel Covers .2 .2

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G J T H N P NUMBER VIN CODES

BELT, DRIVE - ADJUST CAMSHAFT J0659 NOTE: Applicable model years: 1982-86 engine codes 0, J; 1987 engine codes K, M ENGINE CODES 0, J 1.7 ENGINE CODES K, M 1.9 ADD: A- With A/C Engine codes 0, J .2 Engine codes K, M .3

TENSIONER, SERPENTINE J0680 .3 .7 BELT-REPLACE NOTE: Applicable model Team: 1987 OHC4, L4 ADD: A-With A/C .5

COVER AND/OR GASKET, J0770 2.3 CRANKCASE FRONT - REPLACE NOTE: Applicable model year 1987 ADD: A-With A/C .3

COVER,CAMSHAFT J0790 1.3 DRIVE BELT-REPLACE NOTE: Applicable model year: 1987 ADD: A-With A/C .3

BELT, CAMSHAFT DRIVE J0800 - REPLACE NOTE: Applicable model Team: 1982-86 engine codes 0, J; 1987 engine codes K, M ENGINE CODES 0, J 1.8 ENGINE CODES K, M 2.0 ADD: A- With A/C Engine Codes 0, J .2 Engine Codes K, M .3

GEAR,CRANKSHAFT TIMING J0830 2.0 - REPLACE NOTE: Applicable model year: 1987 ADD: A-WitH A/C .3

GEAR, CAMSHAFT TIMING J0840 2.0 - REPLACE NOTE: Applicable model year: 1987 ADD: A-With A/C .3

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G J T H N P NUMBER VIN CODE

MANIFOLD, EXHAUST J0108 1.1 - REPLACE NOTE Applicable model: 1987 w/L-4

SEAL TIMING COVER OIL J0750 2.5 - REPLACE NOTE: Applicable model team: 1987 w/ L-4

SEAL CRANKSHAFT REAR J1120 2.6 MAIN - REPLACE NOTE: Applicable model team: 1984-87 w/ manual trans

BLOCK, ENGINE FITTED J1800 13.3 14.3 - REPLACE NOTE: Applicable model team: 1984-85 J car OHC4, 1985 P car V4 ADD: A-With A/C .4 .5 B-With P/S .2 C-W/Cruise Control .1 D-W/Auto Trans .3 E-W/Turbocharger 1.3 F-To Recondition All Valves 1.6 2.0

ENGINE, PARTIAL/BASIC J1820 10.4 11.4 - REPLACE NOTE: Applicable model years: 1984-85 J car OHC4, 1985 P car V-6 ADD: A-With A/C .4 .5 B-With P/S .2 C-W/Cruise Control .1 D-W/Auto Trans .3 E-W/Turbocharger 1.3 F-To Recondition All Valves 1.6 2.0

ENGINE ASSEMBLY J1880 8.1 7.3 -REPLACE NOTE: Applicable model team: 1984-85 J car OHC4, 1985 P car V4 ADD: A-With A/C .4 .5 B-With P/S .2 C-W/Cruise Control .1 D-W/Auto Trans .3 E-W/Turbocharger 1.3

COVER AND/OR GASKET, ROCKER - REPLACE NOTE: Applicable model team: All w/ codes F, 8 RIGHT BANK J0300 1.2 LEFT BANK J0301 .4 BOTH BANKS J0307 1.5

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G J T H N P NUMBER VIN CODE

COVER AND/OR GASKET, ROCKER - REPLACE ADD: A- With A/C .4

ROCKER ARM - REPLACE NOTE: Applicable model team: All W/codes F,8 RIGHT BANK J0350 1.4 LEFT BANK J0351 .6 BOTH BANKS J0357 1.8 ADD: A- With A/C .4

STUD, ROCKER ARM - REPLACE NOTE: Applicable model team: All W/codes F,8 RIGHT BANK J0380 1.8 LEFT BANK J0381 .8 ADD: A-With A/C .4

SPRING, CAP AND/OR SEAL VALVE-REPLACE NOTE: Applicable model years: All w/codes F,8 RIGHT BANK J0540 1.7 LEFT BANK J0541 .9 BOTH BANKS J0547 2.4 ADD: A- WITH A/C .4

PUSH ROD-REPLACE NOTE: Applicable model team: All W/codes F,8 RIGHT BANK J0580 1.4 LEFT BANK J0581 .6 BOTH BLANKS J0587 1.8 ADD: A- With A/C .4

CAMSHAFT - REPLACE J0850 6.5 NOTE: Applicable model years: 1985 w/ PFI.

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G J T H N P NUMBER VIN CODE

PUMP AND/OR GASKET, J3480 COOLANT - REPLACE 1.3 2.0 NOTE: Applicable model team: 1987 A car L4, J car OHC4. ADD: A- With A/C .3 .3

MAINSHAFT, DISTRIBUTOR J4480 - REPLACE NOTE: Applicable model team: 1982-83 CODES B,G, P .9 CODE 0 1.4

DISTRIBUTOR ASSEMBLY - R&R NOTE: Applicable model team: 1982-83 CODES B,G,P .8 CODE 0 1.3

DISTRIBUTOR ASSEMBLY J4530 - REPLACE NOTE: Applicable model team: 1982-83 CODES B,G,P .8 CODE 0 1.3

SOLENOID, STARTER MOTOR J4580 - REPLACE NOTE: Applicable model years: (OHC-4 "J" series) 1986-1987. (L-4 "F" series) 1986 INC. 1.8L & 2.0L including turbo (J series). Removal procedure includes blower motor removal, disconnect starter wires, remove upper starter bolt, rear starter brace, raise vehicle, remove transaxle strut (auto trans) and lower starter bolt, lower vehicle and remove starter through blower motor opening. L-4 1.1 OHC-4 1.6

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G J T H N P NUMBER VIN CODE

DRIVE ASSEMBLY, STARTER J4600 MOTOR - REPLACE NOTE: Applicable model team: (OHC-4 'J' series) 1986-1987. (L4 'F' series) 1986. INC: 1.8L & 2.OL including turbo (J series). Removal procedure includes blower motor removal, disconnect starter wires, remove upper starter bolt, rear starter brace, raise vehicle, remove transaxle strut (auto trans) and lower starter bolt, lower vehicle and remove starter through blower motor opening. L4 OHC-4 1.7 L-4 1.2

MOTOR ASSEMBLY, STARTER J4620 - R&R NOTE: Applicable model team: (OHC4 'J' series) 1986-1987. (L4 'F' series) 1986. INC: 1.8L & 2.OL including turbo (J series). Removal procedure includes blower motor removal, disconnect starter wires, remove upper starter bolt, rear starter brace, raise vehicle, remove transaxle strut (auto trans) and lower starter bolt, lower vehicle and remove starter through blower motor opening. OHC-4 1.5 L-4 1.0

MOTOR ASSEMBLY, STARTER J4640 - REPLACE NOTE: Applicable model team: (OHC4 'J' series) 1986-1987. L4 ('F' series) 1986. INC: 1.8L & 2.OL including turbo (J series). Removal procedure includes blower motor removal, disconnect starter wires, remove upper starter bolt rear starter brace, raise vehicle, remove transaxle strut (auto trans) and lower starter bolt, lower vehicle and remove starter through blower motor opening. L-4 1.0 OHC-4 1.5

ELECTRONICALLY CONTROLED EMISSIONS AND FUEL SYSTEM - REPLACE NOTE: Applicable model year 1987 SENSOR THROTTLE POSITION J6374 1.1 1.1

COVER AND/OR GASKET, K6540 2.9 VALVE BODY - REPLACE NOTE: Applicable model team:1986-1987

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G J T H N P NUMBER VIN CODE

LAMP ASSEMBLY - REPLACE NOTE: Applicable model years: 1986-1987 STOP, HIGH LEVEL N1600 .2 ADD: A- W/Rear Spoiler .3

RELAY - REPLACE NOTE: Applicable model year 1987 FOG LAMP N2856 .2

INSTRUMENT PANEL CLUSTER COMPONENTS(DIGITAL/ELECTRONIC) - REPLACE INC. Diagnosis. NOTE: Applicable model years; 1986-1987 MODULE, DRIVER N4172 .3 INFORMATION CENTER DISPLAY

DIMMER, INSTRUMENT PANEL LAMP (AUTOMATIC) - REPLACE N1990 .3 .8 .3 NOTE: Applicable model team: (P and F series) 1985-1987 (H series) 1987. NOTE: Also referred to as 'ILLUMINATION CONTROL RELAY' ILLUMINATION CONTROL DISPLAY MODULE'.

GRILLE RADIO SPEAKER - R&R OR REPLACE FRONT RIGHT R0910 .8 LEFT R0911 .8 BOTH R0918 .8

ACTUATOR MOTOR, ELECTRIC FUEL FILLER DOOR LOCK - R&R OR REPLACE R4060 .4 NOTE: Applicable model years: 1986-1987

MIRROR, OUTSIDE REAR VIEW - REPLACE NOTE: Applicable model team: All REMOTE CONTROL RIGHT R3280 .7 1.4 .6 .7

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G J T H N P NUMBER VIN CODE

DUCT ASSEMBLY, DEFROSTER - REPLACE A/C D1432 1.5 NOTE: Applicable model year 1986

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.