COOLING SYSTEM LEAK AT RADIATOR HOSES-NEW P/N CLAMP. Pontiac Tempest (Canada) 1987

For 1990-2009 cars

# COOLING SYSTEM LEAK AT RADIATOR HOSES-NEW P/N CLAMP

SOME OF THE ABOVE VEHICLES MAY HAVE LOOSE RADIATOR HOSES THAT ARE LEAKING COOLANT. THIS IS DUE TO THE HOSE CLAMPS HAVING INSUFFICIENT CLAMPING FORCE. THIS CONDITION MAY BE REPAIRED BY REPLACING THE EXISTING HOSE CLAMPS WITH THE FOLLOWING SERVIVCE PART. PART NUMBER PART NAME _______________ ______________ 10056745 HOSE CLAMP THIS CLAMP CAN BE USED AS A SERVICE PART ON BOTH UPPER AND LOWER RADIATOR HOSES. THE SUBJECT CONDITION MAY BE PRESENT ON ANY VEHICLE BUILT PRIOR TO THE FOLLOWING BREAKPOINTS. LINDEN -- E 291533 WILMINGTON -- Y 284984 USE APPLICABLE LABOR OPERATION AND TIME.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.