CATALYTIC CONVERTER EXHAUST ODOR-NEW P/N AVAILABLE. Pontiac Tempest (Canada) 1987

For 1990-2009 cars

# CATALYTIC CONVERTER EXHAUST ODOR-NEW P/N AVAILABLE

CATALYTIC CONVERTOR ODOR

1987 6000 VEHICLES EQUIPPED WITH 2.8L V-6 ENGINE (VIN W)

Some 1987 6000 vehicles may exhibit a higher than normal catalytic converter odor during vehicle operation. This odor condition can be reduced by installing a service catalytic converter, part number 25104019. The 1988 vehicle has the new design already installed.

Use applicable Labor Operation Numbers and Labor Time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.