For 1990-2009 cars

### Removal Procedure

1. Remove the case side cover. Refer to Control Valve Body Cover Replacement .
2. Disconnect the transaxle wiring harness.
3. Remove the oil pump. Refer to Oil Pump Replacement .
4. Remove the torque converter clutch PWM solenoid (325).

### Installation Procedure

1. Install the torque converter clutch PWM solenoid (325).
2. Connect the transaxle wiring harness.
3. Install the oil pump. Refer to Oil Pump Replacement .
4. Install the case side cover. Refer to Control Valve Body Cover Replacement .