For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Open the third seat passenger side arm rest cover.
3. Using your finger, release and remove the rear quarter trim panel with the third seat audio control from the trim panel.
4. Release the locking tabs using a flat-bladed tool and remove the third seat audio control from the rear quarter trim panel.
5. Disconnect the electrical connector from the third seat audio control.

### Installation Procedure

1. Install the third seat audio control to the rear quarter trim panel.
2. Press the third seat audio control until it locks into place.
3. Connect the electrical connector to the third seat audio control.
4. Install the rear quarter trim panel with the third seat audio control to the trim panel.
5. Connect the negative battery cable.