For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer Rear System Check performed? | -- | Go to Step 2 | Go to Wiper/Washer Rear System Check
2 |

1. Disconnect the rear wiper/washer switch connector C1.
2. Turn the ignition switch to RUN.

Is the wiper on?

--

Go to Step 4

Go to Step 3

3 | Replace the rear wiper/washer switch. Is the replacement complete? | -- | Go to Wiper/Washer Rear System Check | --
4 | Check for a short to voltage in CKT 391 or CKT 392. Is a short to voltage present? | -- | Go to Step 5 | Go to Step 6
5 | Repair the short to voltage in CKT 391 or CKT 392. Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
6 | Replace the rear wiper motor. Refer to Rear Window Wiper Motor Replacement . Is the replacement complete? | -- | Go to Wiper/Washer Rear System Check | --