For 1990-2009 cars

# February, 2000 Labor Time Guide Updates

Subject: | February, 2000 Labor Time Guide Updates

Models: | 1994-2000 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

Important: Please retain any changes made to the A, B, D and L Car Labor Time Guides as these vehicles have been discontinued since 1997 and the Labor Time Guides will not be republished. Changes to the P/H Truck Chassis should also be retained. The vehicle was discontinued in December, 1998. Please note: Labor Time Guides for these discontinued vehicles will not be republished.

#### LTG Update - C/K-New Body Style--Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
INJECTOR, SEQUENTIAL CENTRAL PORT FUEL - REPLACE

- NOTE: Applies to V6 Only

- POLICY: E

ONE | R | J5550 | -- | -- | -- | -- | -- | 1.7 | 1.7
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

--

0-.3

0-.3

REGULATOR AND/OR GASKETS, FUEL PRESSURE - REPLACE | R | J5560 |  |  |  |  |  |  |
EXC 4.3L |  |  | -- | -- | -- | -- | -- | 0.2 | 0.2
4.3L |  |  | -- | -- | -- | -- | -- | 1.7 | 1.7
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
ACCUMULATOR, 1-2 - R&R OR REPLACE

- NOTE: Applies to 4L60E

R

K6506

--

--

--

--

--

0.9

0.9

REACTION GEAR SET - REPLACE

- No Change to "INCs"

- NOTE: Applies to 4L60E

K7285

C TRUCK |  |  | -- | -- | -- | -- | -- | 6.1 | 6.1
K TRUCK | R |  | -- | -- | -- | -- | -- | 7.2 | 7.2
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
MODULE, PULSE WIPER CONTROL - REPLACE | N | N3570 | -- | -- | -- | -- | -- | 0.8 | 0.8
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

--

0-.3

0-.3

PRE-DELIVERY INSPECTION - BASE TIME | R | Z7000 |  |  |  |  |  |  |
PICKUP |  |  | -- | -- | -- | -- | -- | 1.2 | 1.2
YUKON/TAHOE |  |  | -- | -- | -- | -- | -- | -- | 1.4
SUBURBAN/YUKON XL |  |  | -- | -- | -- | -- | -- | -- | 1.4
ADD:

- A- To Install Camper Type Exterior Mirrors (DF2, 9F8)

--

--

--

--

--

0.4

0.4

B- To Install Senior West Coast Type Exterior Mirrors (DG5) |  |  | -- | -- | -- | -- | -- | 0.4 | 0.4
C- To Install Running Boards | R |  | -- | -- | -- | -- | -- | -- | 2.0
*IND: N - New/R - Revised

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
FLYWHEEL (MANUAL TRANSMISSION) - REPLACE

- PART GP: 0.666

- POLICY: D

- NOTE: Applies to Engine Codes F, P, S

J1420

C TRUCK |  |  |  |  |  |  |  |  |
EXC 3500 HD |  |  | 2.5 | 2.5 | 2.5 | 2.5 | 2.5 | 2.5 | 2.5
3500 HD |  |  | 2.8 | 2.8 | 2.8 | 2.8 | 2.8 | 2.8 | 2.8
K TRUCK | R |  | 3.3 | 3.3 | 3.8 | 3.8 | 3.8 | 3.8 | 3.8
ADD:

- A- To Replace Clutch Pilot Bearing

R

0.2

0.2

0.1

0.1

0.1

0.1

0.1

MOUNT, ENGINE - REPLACE

- PART GP: 0.027

- NOTE: For rear center mount, see Trans. Section.

- POLICY: D

- NOTE: Applies to Engine Codes F, P, S

RIGHT |  | J1500 |  |  |  |  |  |  |
C TRUCK |  |  | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7
K TRUCK | R |  | 3.1 | 3.1 | 3.1 | 3.1 | 3.1 | 3.1 | 3.1
LEFT |  | J1501 |  |  |  |  |  |  |
C TRUCK |  |  | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7
K TRUCK | R |  | 3.1 | 3.1 | 3.1 | 3.1 | 3.1 | 3.1 | 3.1
BOTH |  | J1507 |  |  |  |  |  |  |
C TRUCK |  |  | 1.0 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
K TRUCK | R |  | 3.4 | 3.4 | 3.4 | 3.4 | 3.4 | 3.4 | 3.4
No Change to "ADD" Condition |  |  |  |  |  |  |  |  |
LINE AND/OR HOSE, ENGINE OIL COOLER - REPLACE

- PART GP: 1.097

- NOTE: No Change to Labor Operation J3176

BOTH |  | J3177 |  |  |  |  |  |  |
7.4L |  |  | 0.6 | 0.6 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
EXC 7.4L AND DIESEL |  |  | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6
DIESEL | R |  | 1.3 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3
No Change to "ADD" Condition |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - F Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
MOUNT, ENGINE - REPLACE

- NOTE: Applies to Engine Code K

RIGHT | N | J1500 | -- | -- | 1.6 | 1.6 | 1.6 | 1.6 | 1.6
LEFT | N | J1501 | -- | -- | 1.4 | 1.4 | 1.4 | 1.4 | 1.4
BOTH | N | J1507 | -- | -- | 2.1 | 2.1 | 2.1 | 2.1 | 2.1
*IND: N - New/R - Revised

#### LTG Update - G Van Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96-F | 96-1 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | T | V | W | X | Y
GENERATOR ASSEMBLY - REPLACE

- PART GP: 2.275

J4100

EXC 7.4L AND DIESEL | R |  | 0.5 | 0.5 | 0.5 | 1.2 | 1.2 | 1.2 | 1.2 | 1.2
7.4L |  |  | 0.5 | 0.5 | 0.5 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6
DIESEL |  |  | 1.1 | 1.1 | 1.1 | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

*IND: N - New/R - Revised

#### LTG Update - H Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
HOUSING, CRANKSHAFT REAR OIL SEAL - REPLACE

- PART GP: 0.137

- NOTE: For check and adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

J1080

ENGINE CODE K | R |  | -- | 4.6 | 4.6 | 5.6 | 5.6 | 5.6 | 5.6
ENGINE CODE 1 |  |  | -- | -- | 4.6 | 4.6 | 4.9 | 4.9 | 4.9
*IND: N - New/R - Revised

#### LTG Update - K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
COVER AND/OR GASKET, TIMING - REPLACE

- NOTE: Applies to Engine Code 9, Y

R

J0780

1.5

1.5

1.5

1.5

1.6

1.6

1.6

No Change to "ADD" Condition |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - Ksp Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
MOTOR AND/OR FAN, BLOWER - R&R OR REPLACE

- PART GP: 9.275

A/C |  | D1322 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9 | 4.7
A/C REAR | N | D1325 | -- | -- | -- | 0.9 | 0.9 | 0.9 | 3.0
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
CABLES, BATTERY - REPLACE

- PART GP: 2.341 and 2.342

POSITIVE |  |  |  |  |  |  |  |  |
BATTERY TO STARTER |  | N0120 |  |  |  |  |  |  |
ENGINE CODE B |  |  | 0.9 | 0.9 |  |  |  |  |
ENGINE CODE 9, Y | R |  | 1.1 | 1.9 | 1.9 | 1.9 | 1.9 | 1.9 | 1.9
INC: Cable to generator and junction box | N |  |  |  |  |  |  |  |
NOTE: No Change to Labor Operations N0123 through N0181 |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - S/T Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
PANEL, CONSOLE TRIM - REPLACE

- NOTE: Applies to roof console only

FRONT | N | C2842 | -- | -- | -- | 0.6 | 0.6 | 0.6 | 0.6
*IND: N - New/R - Revised

#### LTG Update - U/X Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
FENDER - CORROSION PERFORATION REPAIR |  |  |  |  |  |  |  |  |
RIGHT | N | S5090 | -- | -- | -- | 1.5 | 1.5 | 1.5 | 1.5
LEFT | N | S5091 | -- | -- | -- | 1.5 | 1.5 | 1.5 | 1.5
*IND: N - New/R - Revised