For 1990-2009 cars

### Removal Procedure

1. Position the sunroof in the fully closed position.
2. Remove the headliner. Refer to Headlining Trim Panel Replacement In Interior Trim.
3. Push the module express module towards the center of the vehicle in order to unsnap the express module from the sunroof module.
4. Disconnect the electrical connector from the express module
5. Remove the express module from the sunroof.

### Installation Procedure

1. Install the express module to the sunroof.
2. Connect the electrical connector to the express module.
3. Snap the express module into the sunroof module.
4. Install the headliner. Refer to Headlining Trim Panel Replacement In Interior Trim.
5. Check the operation of the sunroof.