For 1990-2009 cars

### Removal Procedure

1. Loosen/remove the wheel nut caps.
2. Use a flat-bladed tool in order to pry the edge of the wheel cover out.
3. Use your fingers in order to pull the wheel cover off of the wheel.
4. Place the wheel cover down with the finished surface facing up. Do NOT place anything on top of the wheel cover.

### Installation Procedure

1. Install the wheel cover.
2. Install the wheel nut caps.

Tighten
Tighten the wheel nut caps to 3 N·m (27 lb in).