For 1990-2009 cars

## Engine Mount Strut Bracket Replacement Upper Radiator Support

### Removal Procedure

1. Remove the engine mount strut from the engine mount strut bracket at the upper radiator support. Refer to Engine Mount Strut Replacement .
2. Remove the engine mount strut bracket bolts from the engine mount strut bracket.
3. Remove the engine mount strut bracket from the upper radiator support.

### Installation Procedure

1. Position the engine mount strut bracket over the upper radiator support. Ensure that the engine mount strut bracket and the engine mount strut are aligned to the proper holes of the upper radiator support.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the engine mount strut bracket bolts to the engine mount strut bracket.

Tighten
Tighten the engine mount strut bracket bolts to 28 N·m (21 lb ft).

3. Install the engine mount strut to the engine mount strut bracket at the upper radiator support. Refer to Engine Mount Strut Replacement .

## Engine Mount Strut Bracket Replacement Left Side

### Removal Procedure

1. Remove the left engine mount strut from the left engine mount strut bracket. Refer to Engine Mount Strut Replacement .
2. Remove the thermostat housing. Refer to Engine Coolant Thermostat Replacement in Engine Cooling.
3. Remove the engine mount strut bracket bolts from the left engine mount strut bracket to the cylinder head.
4. Remove the left engine mount strut bracket.

### Installation Procedure

1. Install the left engine mount strut bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the engine mount strut bracket bolts through the engine mount strut bracket to the cylinder head.

Tighten
Tighten the engine mount strut bracket bolts to 70 N·m (52 lb ft).

3. Install the thermostat housing. Refer to Engine Coolant Thermostat Replacement in Engine Cooling.
4. Install the left engine mount strut to the left engine mount strut bracket. Refer to Engine Mount Strut Replacement .

## Engine Mount Strut Bracket Replacement Right Side

### Removal Procedure

1. Disconnect the battery ground (negative) cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the right engine mount strut from the right engine mount strut bracket. Refer to Engine Mount Strut Replacement .
3. Remove the engine oil cooler coolant line bracket bolt. Refer to Oil Cooler Hose/Pipe Replacement .
4. Remove the engine wiring harness bracket bolt.
5. Remove the air conditioning compressor mounting bolts and set the compressor aside. Refer to Compressor Replacement in HVAC Systems - Manual.
6. Remove the vertical engine mount strut bracket bolt from the right engine mount strut bracket.
7. Remove the lower engine mount strut bracket bolt from the right engine mount strut bracket.
8. Remove the right engine mount strut bracket.

### Installation Procedure

1. Position the right engine mount strut bracket over the pin locator.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the lower engine mount strut bracket bolt through the right engine mount strut bracket into the cylinder block.

Tighten
Tighten the engine mount strut bracket bolt to 50 N·m (37 lb ft).

3. Install the vertical engine mount strut bracket bolt through the right engine mount strut bracket to the cylinder head.

Tighten
Tighten the engine mount strut bracket bolt to 50 N·m (37 lb ft).

4. Install the air conditioning compressor. Refer to Compressor Replacement in HVAC Systems - Manual.
5. Install the engine wiring harness bracket bolt.

Tighten
Tighten the engine wiring harness bracket bolt to 13 N·m (110 lb in).

6. Install the engine oil cooler coolant line bracket bolt. Refer to Oil Cooler Hose/Pipe Replacement .
7. Install the right engine mount strut to the right engine mount strut bracket. Refer to Engine Mount Strut Replacement .
8. Connect the battery ground (negative) cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.