For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the tilt lever. Refer to Tilt Lever Replacement - On Vehicle .
3. Remove the steering wheel. Refer to Steering Wheel Replacement .
4. Remove the ignition lock cylinder. Refer to Ignition Lock Cylinder Replacement - On Vehicle .
5. Remove the steering column trim covers. Refer to Steering Column Trim Covers - Disassemble - Off Vehicle .
6. Remove the lock module assembly. Refer to Electronic Column Lock Module - Disassemble - Off Vehicle .

### Installation Procedure

1. Install the lock module assembly. Refer to Electronic Column Lock Module - Assemble - Off Vehicle .
2. Install the steering column trim covers. Refer to Steering Column Trim Covers - Assemble - Off Vehicle .
3. Install the ignition lock cylinder. Refer to Ignition Lock Cylinder Replacement - On Vehicle .
4. Install the steering wheel. Refer to Steering Wheel Replacement .
5. Install the tilt lever. Refer to Tilt Lever Replacement - On Vehicle .
6. Enable the SIR system. Refer to Enabling the SIR System in SIR.