For 1990-2009 cars

Important: Do not wash the proportioning valve in any cleaning solution. The internal components are lubricated with a special grease.

The proportioning valves are located in the master cylinder. The valves proportion the brake fluid to each caliper or wheel cylinder after a predetermined amount of pressure is reached. This feature maintains a proper brake force balance during all braking maneuvers.