For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Inspect the PWR SEAT/PSD circuit breaker. Is the PWR SEAT/PSD circuit breaker open? | -- | Go to Step 2 | Go to Step 3
2 |

1. Repair the short to ground in CKT 340.
2. Inspect the system.

Is the repair complete?

--

Go to Power Seats System Check

--

3 | Use a test lamp in order to backprobe between S302 and ground. Does the test lamp light? | -- | Go to Step 4 | Go to Step 5
4 |

1. Repair the following conditions in CKT 550 between S333 and G301:

• | A poor connection

• | An open

2. Inspect the system.

Is the repair complete?

--

Go to Power Seats System Check

--

5 |

1. Repair the following conditions in CKT 340 between S302 and the fuse block:

• | A poor connection

• | An open

2. Inspect the system.

Is the repair complete?

--

Go to Power Seats System Check

--