For 1990-2009 cars
Engine Controls Components
Power, Ground, MIL, DLC
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

Output Driver Modules (ODMs) are used by the PCM to turn on many of the current-driven devices that are needed to control various engine and Transaxle functions. Each ODM is capable of controlling up to 7 separate outputs by applying ground to the device which the PCM is commanding on. Unlike the Quad Driver Modules (QDMs) used in prior model years, ODMs have the capability of diagnosing each output circuit individually. DTC P1671 set indicates an improper voltage level on the output circuit that controls the Malfunction Indicator Lamp (MIL).

### Conditions for Setting the DTC

• | Ignition is ON.

• | An improper voltage level has been detected on ODM A output 1 (the MIL driver circuit).

• | Above conditions for at least 30 seconds.

### Action Taken When the DTC Sets

• | The PCM will not illuminate the malfunction indicator lamp (MIL).

• | The PCM will store conditions which were present when the DTC set as Failure Records data only. This information will not be stored as Freeze Frame data.

### Conditions for Clearing the MIL/DTC

• | A History DTC will clear after 40 consecutive warm-up cycles have occurred without a malfunction.

• | The DTC can be cleared by using the scan tool Clear Info function.

### Diagnostic Aids

Check for the following conditions:

• | Poor connection at PCM. Inspect harness connectors for backed out terminals, improper mating, broken locks, improperly formed or damaged terminals, and poor terminal to wire connection.

• | Damaged harness. Inspect the wiring harness for damage. If the harness appears to be OK, disconnect the PCM, turn the ignition ON and observe a voltmeter connected to the MIL driver circuit at the PCM harness connector while moving connectors and wiring harnesses related to the MIL. A change in voltage will indicate the location of the fault.

Reviewing the Fail Records vehicle mileage since the diagnostic test last failed may help determine how often the condition that caused the DTC to be set occurs. This may assist in diagnosing the condition.

### Test Description

The number(s) below refer to the step number(s) on the Diagnostic Table:

1. Normally, ignition feed voltage should be present on the output control circuit with the PCM disconnected and the ignition turned on.

2. Checks for a shorted component or a short to battery positive voltage on the output control circuit. Either condition would result in a measured current of over 1.5 amps. Also checks for a component that is causing an open circuit while being operated, resulting in a measured current of 0 amps.

3. Checks for a faulty MIL bulb.

4. This vehicle is equipped with a PCM which utilizes an Electrically Erasable Programmable Read Only Memory (EEPROM). When the PCM is being replaced, the new PCM must be programmed. Refer to Powertrain Control Module Replacement/Programming .

#### DTC P1671 - MIL Control Circuit

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain OBD System Check performed? | -- | Go to Step 2 | Go to the Powertrain On Board Diagnostic (OBD) System Check
2 |

1. Turn OFF the ignition switch.
2. Disconnect the PCM.
3. Turn ON the ignition switch.
4. Using a J 39200 Digital Multimeter, measure voltage between the MIL output control circuit at the PCM harness connector and ground.

Is the voltage near the specified value?

B+

Go to Step 3

Go to Step 6

3 |

1. Set up Digital Multimeter to measure current (10 amp range).
2. Measure current between the MIL output control circuit and ground.
3. Monitor the current reading on the Digital Multimeter for at least 2 minutes.

Does the current reading remain between the specified values?

0.05-1.5 Amps

Go to Step 11

Go to Step 4

4 |

1. Turn OFF the ignition switch.
2. Disconnect the instrument panel (leave the PCM disconnected).
3. Turn ON the ignition switch.
4. Using Digital Multimeter, measure voltage between the MIL output control circuit and ground.

Is the voltage at the specified value?

0.0V

Go to Step 10

Go to Step 5

5 | Locate and repair short to voltage in the MIL output control circuit. Refer to Wiring Repairs in Wiring Systems. Is the action complete? | -- | Go to Step 15 | --
6 | Check the ignition feed fuse for the instrument panel indicators. Is the fuse blown? | -- | Go to Step 7 | Go to Step 8
7 |

1. Locate and repair short to ground in ignition feed circuit for the instrument panel indicators. Refer to Wiring Repairs in Wiring Systems.
2. Replace the fuse.

Is the action complete?

--

Go to Step 15

--

8 |

1. Disconnect the instrument cluster.
2. Turn ON the ignition switch.
3. Measure voltage between the ignition feed circuit for the instrument cluster indicators and ground.

Is the voltage near the specified value?

B+

Go to Step 9

Go to Step 13

9 |

1. Check the MIL output control circuit for an open or a short to ground.
2. If a problem is found, repair the MIL output control circuit. Refer to Wiring Repairs in Wiring Systems.

Was a problem found?

--

Go to Step 15

Go to Step 10

10 |

1. Check the MIL output control circuit and the instrument panel indicators ignition feed circuit for a poor connection at the instrument panel and at the PCM.
2. If a problem is found, replace the malfunctioning terminal(s). Refer to Connector Repairs in Wiring Systems.

Was a problem found?

--

Go to Step 15

Go to Instrument Panel in Electrical Diagnosis

11 |

1. Turn OFF the ignition switch, reconnect the PCM and disconnect the instrument cluster.
2. Turn ON the ignition switch.
3. Connect a test light between the MIL output control circuit and the ignition feed circuit at the instrument panel harness connector.
4. Using the scan tool outputs test function, cycle the MIL ON and OFF.

Does the test light flash ON and OFF?

--

Go to Diagnostic Aids

Go to Step 12

12 |

1. Check the MIL output control circuit for a poor connection at the PCM.
2. If a problem is found, replace the damaged terminal. Refer to Connector Repairs in Wiring Systems.

Was a problem found?

--

Go to Step 15

Go to Step 14

13 | Locate and repair open in ignition feed circuit to the I/P indicators. Refer to Wiring Repairs in Wiring Systems. Is the action complete? | -- | Go to Step 15 | --
14 | Important: : The replacement PCM must be programmed. Refer to Powertrain Control Module Replacement/Programming . Replace the PCM. Is the action complete? | -- | Go to Step 15 | --
15 |

1. Review and record scan tool Fail Records data.
2. Clear DTCs.
3. Operate the vehicle within Fail Records conditions as noted.
4. Using a scan tool, monitor Specific DTC info for DTC P1671 until the DTC P1671 test runs.

Note test result, does scan tool indicate DTC P1671 failed this ignition?

--

Go to Step 2

System OK