For 1990-2009 cars

### Removal Procedure

1. Pull the windshield garnish molding from the A-pillar in order to disengage the retaining tabs and clips.
2. Remove the windshield garnish molding from the A-pillar.

### Installation Procedure

1. Align the windshield garnish molding to the headliner and the holes in the A-pillar.
2. Press on the windshield garnish molding in order to engage the retaining tabs and clips.