For 1990-2009 cars

### Removal Procedure

1. Remove the reservoir hose clamp and the hose at the radiator overflow fitting.
2. Remove the mounting clips to the reservoir.
3. Remove the coolant reservoir.
4. Clean the coolant reservoir with soap and water. Rinse with clean water.

### Installation Procedure

1. Install the coolant reservoir.
2. Install the mounting clips to the reservoir.
3. Lubricate the reservoir hose with clean water. Route the hose up to the radiator overflow fitting.
4. Install the clamp to the reservoir hose.
5. Refill the coolant reservoir. Refer to Cooling System Draining and Filling .