For 1990-2009 cars

1. Inspect the components that are still on the transmission case for the following conditions:

• | Loose, cross-threaded, or damaged oil cooler pipe fittings

• | A loose, missing, or damaged transmission name plate

2. Inspect the transmission case for the following conditions:

• | Gasket sealing surfaces that are damaged or which have porosity

• | Bolt or screw holes that are stripped or damaged (repair with a thread insert)

• | Damaged or porous case oil passages

• | Damaged snap ring grooves or housing splines

• | Loose, missing, or damaged band anchor pins

• | Damaged or porous case surfaces

• | Plugged drain back holes for the torque converter oil seal

3. Inspect the components that are still on the transmission case for the following conditions:

• | A loose, plugged, or damaged transmission vent assembly

• | A loose, cross-threaded, or damaged oil pressure test hole plug

• | A damaged transmission electrical connector or seal