For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door outside handle. Refer to Sliding Door Outside Handle Replacement in Doors.
2. Remove the lock cylinder retainer from the sliding door outside handle.
3. Remove the sliding door lock cylinder from the sliding door outside handle.

### Installation Procedure

1. Install the sliding door lock cylinder to the sliding door outside handle.
2. Install the lock cylinder retainer to the sliding door outside handle.
3. Install the sliding door outside handle. Refer to Sliding Door Outside Handle Replacement in Doors.