For 1990-2009 cars

## Fastener Tightening Specifications L82

#### Fastener Tightening Specifications

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Accelerator Control Cable Bracket Bolt | 14 | -- | 125
Accelerator Control Cable Bracket Nut | 10 | -- | 89
Camshaft Position Sensor Bolt | 10 | -- | 89
Camshaft Sprocket Bolt | 110 | 81 | --
Camshaft Thrust Plate Bolt | 10 | -- | 89
Connecting Rod Cap Nut | 20 +75° | 15 +75° | --
Coolant Drain Plug | 19 | 14 | --
Coolant Outlet Bolt | 25 | 18 | --
Coolant Pump Bolt | 10 | -- | 89
Coolant Pump Pulley Bolt | 25 | 18 | --
Crankshaft Balancer Bolt | 103 | 76 | --
Crankshaft Oil Deflector Nut | 25 | 18 | --
Crankshaft Position Sensor Bolt - Front Cover | 10 | -- | 89
Crankshaft Position Sensor Bolt - Side of Blocks | 11 | -- | 98
Cylinder Head Bolt | 60 +95° | 44 +95° | --
EGR Adapter Pipe to Exhaust Manifold Nut | 25 | 18 | --
EGR to Adapter Pipe Bolt | 25 | 18 | --
Electronic Ignition Control Module Bracket Bolt | 25 | 18 | --
Electronic Ignition Control Module Bracket Nut | 25 | 18 | --
Engine Coolant Temperature Sensor | 23 | 17 | --
Engine Mount Bracket Bolt | 58 | 43 | --
Engine Mount to Bracket Nut | 47 | 35 | --
Engine Mount to Frame Bracket Nut | 43 | 32 | --
Engine Mount Strut Nut | 48 | 35 | --
Engine Mount Strut Bracket Bolt - Engine Right Side | 50 | 37 | --
Engine Mount Strut Bracket Bolt - Engine Left Side | 70 | 52 | --
Engine Mount Strut Bracket Bolt - Upper Radiator Support | 26 | 19 | --
Exhaust Crossover Pipe Nut | 25 | 18 | --
Exhaust Crossover Pipe Heat Shield Bolt | 10 | -- | 89
Exhaust Manifold Nut | 16 | 12 | --
Exhaust Manifold Heat Shield Bolt | 10 | -- | 89
Exhaust Manifold Stud | 16 | 12 | --
Flywheel Bolt | 83 | 61 | --
Front Cover Bolt - Large | 47 | 35 | --
Front Cover Bolt - Small | 21 | 15 | --
Fuel Injector Rail Bolt | 10 | -- | 89
Fuel Pipe Bracket Bolt | 50 | 37 | --
Fuel Pipe Bracket Stud | 50 | 37 | --
Fuel Pipe Fitting | 17 | 13 | --
Fuel Pipe Retaining Clip Bolt | 10 | -- | 89
Generator Bracket Bolt | 50 | 37 | --
Heater Inlet Pipe Nipple | 30 | 22 | --
Heater Inlet Pipe Nut | 25 | 18 | --
Heater Inlet Pipe Stud | 25 | 18 | --
Knock Sensor | 19 | 14 | --
Lower Intake Manifold Bolt | 13 | -- | 115
MAP Sensor Bolt | 4 | -- | 36
Oil Gallery Plug - 1/4 in | 19 | 14 | --
Oil Gallery Plug - 3/8 in | 33 | 24 | --
Oil Filter | 13 | -- | 115
Oil Filter By-pass Plug | 19 | 14 | --
Oil Filter Fitting | 39 | 29 | --
Oil Filter Cooler Connector | 50 | 37 | --
Oil Level Indicator Assembly Bolt | 25 | 18 | --
Oil Level Sensor | 10 | -- | 89
Oil Pan Retaining Bolt | 25 | -- | 18
Oil Pan Side Bolt | 50 | 37 | --
Oil Pan Drain Plug | 25 | 18 | --
Oil Pressure Switch | 13 | -- | 115
Oil Pump Bolt | 41 | 30 | --
Oil Pump Cover Bolt | 10 | -- | 89
Oil Pump Drive Assembly Bolt | 36 | 27 | --
Rear Engine Lift Bracket Bolt | 50 | 37 | --
Rocker Arm Bolt | 10 +30° | -- | 89 +30°
Rocker Cover Retaining Bolt (Finger Tighten All Bolts First) | 10 | -- | 89
Spark Plug | 20 | 15 | --
Throttle Body Bolt | 25 | 18 | --
Timing Chain Dampener Bolt | 21 | 15 | --
Upper Intake Manifold Bolt | 25 | 18 | --
Upper Intake Manifold Stud | 25 | 18 | --
Valve Lifter Guide Bolt | 10 | -- | 89

## Fastener Tightening Specifications LG8 and LA1

Application | Specification
--- | ---
Metric | English
Accelerator Control Cable Bracket Bolt/Nut | 10 N·m | 89 lb in
Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Camshaft Sprocket Bolt | 140 N·m | 103 lb ft
Camshaft Thrust Plate Screw | 10 N·m | 89 lb in
Connecting Rod Bearing Cap Nut | 20 N·m + 75° | 15 lb ft + 75°
Coolant Drain Plug | 19 N·m | 14 lb ft
Coolant Temperature Sensor | 23 N·m | 17 lb ft
Crankshaft Balancer Bolt | 103 N·m | 76 lb ft
Crankshaft Main Bearing Cap Bolt/Stud | 50 N·m +77° | 37 lb ft + 77°
Crankshaft Oil Deflector Nut | 25 N·m | 18 lb ft
Crankshaft Position Sensor Bolt -- Front Cover | 10 N·m | 89 lb in
Crankshaft Position Sensor Stud -- Side of Engine Block | 11 N·m | 98 lb in
Crankshaft Position Sensor Wiring Bracket Bolt | 27 N·m | 20 lb ft
Cylinder Head Bolt | 60 N·m + 95° | 44 lb ft + 95°
Drive Belt Shield Bolt | 10 N·m | 89 lb in
Drive Belt Tensioner Bolt | 50 N·m | 37 lb ft
EGR Valve to EGR Valve Pipe Bolt | 25 N·m | 18 lb ft
EGR Valve Adapter Pipe to Exhaust Manifold Nut | 25 N·m | 18 lb ft
Engine Flywheel Bolt | 71 N·m | 52 lb ft
Engine Front Cover Bolt -- Large | 55 N·m | 41 lb ft
Engine Front Cover Bolt -- Medium | 47 N·m | 35 lb ft
Engine Front Cover Bolt -- Small | 21 N·m | 15 lb ft
Engine Mount Bracket Bolt | 58 N·m | 43 lb ft
Engine Mount Lower Nut | 43 N·m | 32 lb ft
Engine Mount Strut and Lift Bracket Bolt -- Engine Left Rear | 70 N·m | 52 lb ft
Engine Mount Strut Bolt/Nut | 48 N·m | 35 lb ft
Engine Mount Strut Bracket Bolt -- Upper Radiator Support | 28 N·m | 21 lb ft
Engine Mount Strut Bracket Bolt -- Vehicle Right Side | 50 N·m | 37 lb ft
Engine Mount Upper Nut | 47 N·m | 35 lb ft
Engine Oil Pressure Indicator Switch | 13 N·m | 115 lb in
Engine Wiring Harness Bracket Bolt | 13 N·m | 115 lb in
Exhaust Crossover Pipe Heat Shield Bolt | 10 N·m | 89 lb in
Exhaust Crossover Pipe Nut/Stud | 25 N·m | 18 lb ft
Exhaust Manifold Heat Shield Bolt | 10 N·m | 89 lb in
Exhaust Manifold Nut | 16 N·m | 12 lb ft
Exhaust Manifold Stud | 18 N·m | 13 lb ft
Fuel Feed Pipe to Fuel Injector Rail Nut | 17 N·m | 13 lb ft
Fuel Injector Rail Bolt | 10 N·m | 89 lb in
Fuel Pipe Bracket Bolt/Stud | 50 N·m | 37 lb ft
Fuel Pipe Clip Bolt | 8 N·m | 71 lb in
Fuel Return Pipe to Fuel Injector Rail Nut | 17 N·m | 13 lb ft
Generator Bracket and Front Engine Lift Hook Bolt | 50 N·m | 37 lb ft
Heated Oxygen Sensor | 42 N·m | 31 lb ft
Heater Inlet Pipe Nut | 25 N·m | 18 lb ft
Ignition Coil Bracket Bolt/Nut/Stud | 25 N·m | 18 lb ft
Intake Manifold Coolant Pipe Bolt | 10 N·m | 89 lb in
Knock Sensor | 19 N·m | 14 lb ft
Lower Intake Manifold Bolt - Center

- First Pass

7 N·m

62 lb in

- Final Pass

13 N·m

115 lb in

Lower Intake Manifold Bolt - Corner

- First Pass

13 N·m

115 lb in

- Final Pass

25 N·m

18 lb ft

MAP Sensor Bolt | 5 N·m | 44 lb in
Oil Cooler Connector | 50 N·m | 37 lb ft
Oil Cooler Hose Fitting | 19 N·m | 14 lb ft
Oil Cooler Pipe Bracket Bolt | 10 N·m | 89 lb in
Oil Filter | 13 N·m | 115 lb in
Oil Filter Bypass Hole Plug | 19 N·m | 14 lb ft
Oil Filter Fitting | 39 N·m | 29 lb ft
Oil Gallery Plug -- 1/4 inch | 19 N·m | 14 lb ft
Oil Gallery Plug -- 3/8 inch | 33 N·m | 24 lb ft
Oil Level Indicator Tube Stud | 25 N·m | 18 lb ft
Oil Level Sensor Bolt | 10 N·m | 89 lb in
Oil Pan Bolt | 25 N·m | 18 lb ft
Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pan Side Bolt | 50 N·m | 37 lb ft
Oil Pump Cover Bolt | 10 N·m | 89 lb in
Oil Pump Drive Clamp Bolt | 36 N·m | 27 lb ft
Oil Pump Mounting Bolt | 41 N·m | 30 lb ft
Spark Plug

- Spark Plug - Initial Installation

20 N·m

15 lb ft

- Spark Plug - Reinstallation

15 N·m

11 lb ft

Thermostat Bypass Pipe to Cylinder Head Nut | 25 N·m | 18 lb ft
Thermostat Bypass Pipe to Engine Front Cover Bolt | 12 N·m | 106 lb in
Thermostat Bypass Pipe to Throttle Body Nut | 25 N·m | 18 lb ft
Throttle Body Bolt/Stud | 25 N·m | 18 lb ft
Timing Chain Dampener Bolt | 21 N·m | 15 lb ft
Upper Intake Manifold Bolt/Stud | 25 N·m | 18 lb ft
Valve Lifter Guide Bolt | 10 N·m | 89 lb in
Valve Rocker Arm Bolt | 15 N·m + 30° | 11 lb ft+ 30°
Valve Rocker Arm Cover Bolt | 10 N·m | 89 lb in
Water Outlet Bolt | 25 N·m | 18 lb ft
Water Pump Bolt | 10 N·m | 89 lb in
Water Pump Pulley Bolt | 25 N·m | 18 lb ft