For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Inspect the headlamp and the instrument panel (IP) lamp dimmer switch harness connector for a poor connection. Is there a poor connection? | -- | Go to Step 2 | Go to Step 3
2 |

1. Repair a poor connection on the headlamp switch.
2. Inspect the system.

Is the symptom still present?

--

Go to Step 3

Go to Interior Lamps System Check

3 |

1. Replace the headlamp and IP lamp dimmer switch. Refer to Headlamp Switch Replacement .
2. Inspect the system.

Is the symptom still present?

--

--

Go to Interior Lamps System Check