For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the oil pan. Refer to Oil Pan Replacement .
3. Remove the filter. Refer to Automatic Transmission Fluid Filter and Seal Replacement .
4. Remove the accumulator attaching bolts (131).
5. Remove the manual 2-1 band servo cover bolts (103).
6. Use a large flat-bladed tool in order to gently pry the lube oil pipe retainer (129) from the case.
7. Remove the lube oil pipe (130) from the front differential carrier internal gear lube hole.
8. Remove the accumulator (132).
9. Remove the manual 2-1 band servo cover (104).
10. Remove the manual 2-1 band servo (106-116).
11. Remove the manual 2-1 band servo cover gasket (105).
12. For information on the disassembly and inspection of the accumulator and manual 2-1 band servo, refer to the Transmission/Transaxle/Transfer Case Unit Repair Manual.

### Installation Procedure

1. Install the manual 2-1 band servo cover gasket (105) into the case. Lubricate the manual 2-1 band servo cover gasket with automatic transmission fluid.
2. Install the manual 2-1 band servo (106-116).
3. Install the manual 2-1 band servo cover (104).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the manual 2-1 band servo cover bolts (103).

Tighten
Tighten the manual 2-1 band servo cover bolts (103) to 24 N·m (17 lb ft).

5. Install the accumulator (132).
6. Install the lube oil pipe (130) into the case at the lube hole for the front differential carrier internal gear.
7. Use a flat-bladed tool in order to lock the lube oil pipe retainer (129) into the case.
8. Install the accumulator attaching bolts (131).

Tighten
Tighten the accumulator attaching bolts (131) to 11 N·m (97 lb in).

9. If removed, install a new filter seal.
10. Install the filter. Refer to Automatic Transmission Fluid Filter and Seal Replacement .
11. Install the oil pan. Refer to Oil Pan Replacement .
12. Lower the vehicle.