For 1990-2009 cars

1. Install the 2-1 manual band servo cover seal (105) into the case. Lubricate the 2-1 manual band servo cover seal (105) with automatic transmission fluid.

Notice: Do not damage the 2-1 manual band servo exhaust screen on installation.

2. Install the 2-1 manual band servo assembly (106-116) into the case. Make sure that the 2-1 manual band servo pin engages the 2-1 manual band assembly.
3. Install the accumulator (132-140) and 2-1 manual band servo cover assembly (104) into the case.
4. Install the lube oil pipe and washer assembly (130) through the case and into the lube hole in the differential carrier internal gear.
5. Use a screwdriver in order to lock the lube oil pipe retainer (129) into the case.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the three 2-1 manual band servo cover bolts (103).

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

7. Install the four accumulator cover bolts (131).

Tighten
Tighten the bolts to 12 N·m (106 lb in).