For 1990-2009 cars

### Removal Procedure

1. Open the ashtray.
2. Remove the screws from the IP accessory trim plate.
3. Use a small, flat-bladed tool in order to remove the upper tabs on the IP accessory trim plate from the instrument panel.
4. Disconnect the electrical connectors.
5. Remove the IP accessory trim plate from the instrument panel.

### Installation Procedure

1. Install the IP accessory trim plate to the instrument panel.
2. Connect the electrical connectors.
3. Align the upper tabs of the IP accessory trim plate to the instrument panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the screws to the IP accessory trim plate.

Tighten
Tighten the screws to 2 N·m (18 lb in).

5. Close the ashtray.