For 1990-2009 cars

### Removal Procedure

1. Remove the extension housing. Refer to Case Extension Housing Disassemble .
2. Remove the thrust bearing and the thrust washer.
3. Remove the final drive.
4. Disassemble the final drive. Refer to Case Components Disassemble .
5. Assemble the final drive. Refer to Case Components Assemble .

### Installation Procedure

1. Install the final drive.
2. Install the thrust washer and the thrust bearing.
3. Install the extension housing. Refer to Case Extension Housing Disassemble .
4. Measure the end play. Refer to Case Assembly Inspection .
5. Adjust the fluid level.
6. Inspect for the following:

• | Proper completion of repairs

• | Proper fluid level. Refer to Transmission Fluid Check .

• | Fluid leaks. Refer to Fluid Leak Diagnosis and Repair .