For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement .
2. Remove the bolts/screws from the hood release handle.
3. Remove the hood release handle from the instrument panel.
4. Use a small, flat-bladed tool in order to remove the hood release cable grommet from the brake pedal bracket plate.
5. Remove the hood release cable from the hood latch.
6. Route the hood release cable from the brake pedal bracket plate.
7. Remove the hood release cable and hood release handle from the vehicle.

### Installation Procedure

1. Install the hood release cable and hood release handle to the vehicle.
2. Route the hood release cable to the brake pedal bracket plate panel.
3. Install the hood release cable to the hood latch.
4. Press the hood release cable grommet into place in order to install the grommet to the brake pedal bracket plate.
5. Install the hood release handle to the instrument panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the bolts/screws to the hood release handle.

Tighten
Tighten the bolts/screws to 2 N·m (18 lb in).

7. Install the knee bolster. Refer to Knee Bolster Replacement .