For 1990-2009 cars

# FRONT WINDOW IS INOPERATIVE OR JUMPS WHEN BEING ROLLED UP/DWN

#### SUBJECT: FRONT WINDOW IS INOPERATIVE OR JUMPS WHEN BEING ROLLED UP OR DOWN (INSTALL NEW REGULATOR/MOTOR KIT)

#### MODELS: 1990-95 CHEVROLET LUMINA APV 1990-95 OLDSMOBILE SILHOUETTE 1990-95 PONTIAC TRANS SPORT

********************************************************************* THIS BULLETIN CANCELS AND SUPERSEDES CORPORATE BULLETIN NUMBER 431042. PLEASE DISCARD BULLETIN 431042 (GROUP REFERENCE 10 - BODY). *********************************************************************

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE FRONT WINDOW IS INOPERATIVE OR THE WINDOW JUMPS WHEN ROLLING UP OR DOWN.

#### CAUSE:

INTERNAL MOTOR DETERIORATION OR BROKEN GEAR TEETH ON THE MOTOR.

#### CORRECTION:

INSTALL KIT LISTED BELOW WHICH CONTAINS A NEW REGULATOR AND MOTOR, INSTRUCTION SHEET, GUIDE AND RIVETS FOR ATTACHMENT.

#### PROCEDURE:

AFTER REMOVAL OF THE TRIM PANEL, WATER DEFLECTOR AND WINDOW REGULATOR, AND THE WINDOW REGULATOR HAS BEEN REPLACED, PROCEED AS FOLLOWS:

1. CUT TEMPLATE FROM PAGE 2 OF THE KIT AND LOCATE TO THE TOP EDGE OF DOOR INNER PANEL. (SEE FIGURE 1, ITEM 1 - RIGHT HAND DOOR SHOWN).

2. MAKE SURE THE TEMPLATE CONFORMS TO THE DOOR SURFACE (SEE FIGURE 1, ITEM 2).

3. ALIGN THE REAR EDGE OF THE TEMPLATE AS SHOWN IN FIGURE 1, ITEM 3.

4. DRILL 4.5MM (3/16 IN.) HOLES AS SHOWN ON THE TEMPLATE (SEE FIGURE 1, ITEM 4).

5. IF UP-STOP IS PRESENT, DRILL OUT BOTH RETAINING RIVETS AND DISCARD UP STOP (SEE FIGURE 1, ITEM 5).

6. INSTALL GUIDE ASSEMBLY USING RIVETS SUPPLIED IN KIT.

7. RUN THE WINDOW UP WHILE WATCHING THE REGULATOR ARM MEET THE GUIDE FOR CORRECT CONTACT. IF NECESSARY, BEND BRACKET INBOARD FOR CONTACT.

8. REINSTALL WATER DEFLECTOR AND DOOR TRIM.

#### PARTS INFORMATION:

KIT (RIGHT HAND) P/N 10290932 KIT (LEFT HAND) P/N 10290933

PARTS ARE EXPECTED TO BE AVAILABLE APRIL 1, 1996.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER DESCRIPTION LABOR TIME =============== =========== ==========

C0182 RIGHT HAND 0.9 HR

C0183 LEFT HAND 0.9 HR

FIGURES: 01 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.