For 1990-2009 cars

### Removal Procedure

1. Pull down on the rear headliner trim finish molding in order to disengage the retaining tabs and clips from the retainer.
2. Remove the rear headliner trim finish molding from the retainer in the roof.

### Installation Procedure

1. Align the rear headliner trim finish molding to the retainer in the roof.
2. Press up on the rear headliner trim finish molding in order to engage the retaining tabs and clips.