For 1990-2009 cars

### Removal Procedure

1. Remove the rear quarter window. Refer to Quarter Window Replacement .
2. Remove the pin from the latch bearing.
3. Remove the bearing bushing retaining screw.
4. Disconnect the electrical connector from the actuator.
5. Remove the power rear quarter window actuator retaining screws.
6. Remove the actuator from the vehicle.

### Installation Procedure

1. Install the actuator to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the power rear quarter window actuator retaining screws.

Tighten
Tighten the retaining screws to 10 N·m (89 lb in).

3. Connect the electrical connector from the actuator.
4. Install the bearing bushing retaining screw.

Tighten
Tighten the bearing bushing retaining screw to 2 N·m (18 lb in).

5. Install the pin to the latch bearing.
6. Install the rear quarter window. Refer to Quarter Window Replacement .