For 1990-2009 cars

### Removal Procedure

1. Remove the case extension housing. Refer to Case Extension Housing Disassemble .
2. Remove the output shaft retaining clip at the differential.
3. Remove the output shaft through the left wheel opening.

### Installation

1. Install the output shaft through the left wheel opening.
2. Install the output shaft retaining clip at the differential.
3. Install the case extension housing. Refer to Case Extension Housing Disassemble .
4. Adjust the fluid level.
5. Inspect for the following:

• | Proper completion of repairs

• | Proper fluid level. Refer to Transmission Fluid Check .

• | Fluid leaks. Refer to Fluid Leak Diagnosis and Repair .