For 1990-2009 cars

Problem | Action
--- | ---
The springs are broken or sagging. | Repair as necessary. Refer to Trim Height Inspection .
The stabilizer shaft is loose or disconnected. | Inspect the stabilizer shaft links and insulators for damage. Repair or replace as necessary.

• | For the stabilizer shaft link replacement, refer to Stabilizer Shaft Link Replacement .

• | For the stabilizer shaft insulator replacement, refer to Stabilizer Shaft Insulator Replacement .

The strut dampener is worn. | Repair as necessary. Refer to Strut, Strut Component, and Spring Replacement .
The vehicle is overloaded. | Reduce the vehicle load. Refer to Tire Placard in Maintenance and Lubrication.
The tire pressure(s) is incorrect. | Inflate the tire(s) to proper specifications. Refer to Tire Placard in Maintenance and Lubrication.