For 1990-2009 cars

Table 1: | Cruise Control Module
Table 2: | Cruise Control Release Switch
Table 3: | Stop Lamp Switch C1

#### Cruise Control Module

Connector Part Information |

• | 12065425

• | 10-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 397 | Cruise ON/OFF
B | DK BLU | 84 | Cruise control set/coast switch signal
C | GRY/BLK | 87 | Cruise control resume/accelerate switch signal
D | BRN | 86 | Cruise control release switch output
E | BLK | 1150 | Ground
F | PNK | 739 | Fused cruise feed
G | WHT | 17 | Stop lamp switch signal
H | DK GRN | 83 | Cruise control inhibit input signal
J | WHT | 85 | Cruise control engaged signal
K | DK GRN | 389 | Vehicle speed signal - 4000 pulses per mile

#### Cruise Control Release Switch

Connector Part Information |

• | 12041433

• | 2-Way F Metri-Pack 280 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 86 | Cruise control release switch output
B | PNK | 739 | Fused cruise feed

#### Stop Lamp Switch C1

Connector Part Information |

• | 12033701

• | 2-Way F Metri-Pack 480 Series (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 140 | Fused battery feed
B | WHT | 17 | Stop lamp switch output