For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Open and suitably support the hood.
2. Use J 38778 in order to remove the push-in retainers from the hood insulator.
3. Pull the hood insulator from the tabs in the hood inner panel.
4. Remove the hood insulator from the hood.

### Installation Procedure

1. Align the hood insulator to the hood.
2. Tuck the hood insulator into the tabs in the hood inner panel.
3. Install the push-in retainers to the hood insulator.
4. Close the hood.