For 1990-2009 cars

# SMU-SEC.9J - SIR - REVISED FASTEN. TIGHT. SPEC. FOR SIDE

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 9J - SIR - REVISED FASTENER TIGHTENING SPECIFICATION FOR SIDE IMPACT SENSOR (SIS)

#### MODELS: 1998 CHEVROLET VENTURE 1998 OLDSMOBILE SILHOUETTE 1998 PONTIAC TRANS SPORT

THIS BULLETIN IS BEING ISSUED TO REVISE THE FASTENER TIGHTENING SPECIFICATION (SIDE IMPACT SENSOR - SIS) IN SECTION 9J OF THE SERVICE MANUAL.

STEP 3 IN THE "INSTALLATION PROCEDURE" SHOULD BE CHANGED AS FOLLOWS:

3. INSTALL THE FASTENERS TO THE INFLATABLE RESTRAINT SIDE IMPACT SENSOR.

- TIGHTEN

USE ONLY HAND TOOLS TO TIGHTEN THE FASTENERS TO 10 N.M (89 LB IN). REFER TO FASTENER NOTICE IN CAUTIONS AND NOTICES.

THE "FASTENER TIGHTENING SPECIFICATIONS" TABLE SHOULD ALSO BE CHANGED AS FOLLOWS:

APPLICATION N.M LB FT LB IN ----------- --- ----- -----

INFLATABLE RESTRAINT 10 --- 89 SIDE IMPACT SENSOR (SIS) FASTENERS

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.