For 1990-2009 cars

## Seat Belt Replacement - Center Rear 60/40 Split Bench

### Removal Procedure

1. Remove the rear seat. Refer to Seat Replacement - Rear in Seats.
2. Remove the recliner trim cover. Refer to Seat Back Recliner Cover Replacement - Rear in Seats
3. Remove the rear seat riser. Refer to Seat Riser Replacement - Rear in Seats.
4. Unhook the seat cushion cover retainers from the bottom of the seat frame.
5. Remove the bolts securing the buckle side belts from the seat cushion frame.
6. Remove the buckle side belts (1) from the seat.
7. Remove the bolt securing the mini-buckle (2) from the 60 percent seat cushion frame.

### Installation Procedure

1. Install the bolt securing the mini-buckle (2) to the 60 percent seat cushion frame.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the buckle side belts (1) to the seat.

Tighten
Tighten the mini-buckle bolt to 53 N·m (39 lb ft).

3. Install the bolts securing the buckle side belts (1) to the seat cushion frame.

Tighten
Tighten the rear seat buckle belt bolts to 53 N·m (39 lb ft).

4. Hook the seat cushion cover retainers to the bottom of the seat frame.
5. Install the rear seat riser. Refer to Seat Riser Replacement - Rear in Seats.
6. Install the recliner trim cover. Refer to Seat Back Recliner Cover Replacement - Rear in Seats
7. Install the rear seat. Refer to Seat Replacement - Rear in Seats.

## Seat Belt Replacement - Center Rear 50/50 Split Bench

### Removal Procedure

1. Remove the rear seat. Refer to Seat Replacement - Rear in Seats.
2. Remove recliner trim cover. Refer to Seat Back Recliner Cover Replacement - Rear in Seats
3. Remove the rear seat riser. Refer to Seat Riser Replacement - Rear in Seats.
4. Unhook the seat cushion cover retainers (1) from the bottom of the seat frame.
5. Remove the bolts securing the center buckle belts from the seat cushion frame.
6. Remove the center buckle belts from the seat.

### Installation Procedure

1. Install the center buckle belts to the seat.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts securing the center buckle belts to the seat cushion frame.

Tighten
Tighten the rear seat center belt bolts to 53 N·m (39 lb ft).

3. Hook the seat cushion cover retainers (1) to the bottom of the seat frame.
4. Install the rear seat riser. Refer to Seat Riser Replacement - Rear in Seats.
5. Install the recliner trim cover. Refer to Seat Back Recliner Cover Replacement - Rear in Seats
6. Remove the rear seat. Refer to Seat Replacement - Rear in Seats.

## Seat Belt Replacement - Center Rear Full Bench

### Removal Procedure

1. Remove the rear seat. Refer to Seat Replacement - Rear in Seats.
2. Remove the recliner trim cover. Refer to Seat Back Recliner Cover Replacement - Rear in Seats.
3. Remove the rear seat riser. Refer to Seat Riser Replacement - Rear in Seats.
4. Unhook the seat cushion cover retainers (2) from the bottom of the seat frame.
5. Remove the bolts (3) securing the belts from the seat cushion frame.
6. Remove the center belts (1) from the seat.

### Installation Procedure

1. Install the center belts (1) to the seat.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts (3) securing the center belts to the seat cushion frame.

Tighten
Tighten the rear seat center belt bolts to 53 N·m (39 lb ft).

3. Hook the seat cushion cover retainers (2) to the bottom of the seat frame.
4. Install the rear seat riser. Refer to Seat Riser Replacement - Rear in Seats.
5. Install the recliner trim cover. Refer to Seat Back Recliner Cover Replacement - Rear in Seats.
6. Install the rear seat. Refer to Seat Replacement - Rear in Seats.