For 1990-2009 cars

### Removal Procedure

1. Remove the lumbar handle by pulling the lumbar handle straight off.
2. Remove the lumbar handle cover.

### Installation Procedure

1. Install the lumbar handle cover.
2. Orientate the wide section of the lumbar handle cover to the rear of the seat back.
3. Align the lumbar handle splines with the shaft.
4. Firmly press the lumbar handle until it snaps into place.