For 1990-2009 cars

### Removal Procedure

Important: The front and rear washer pump replacement procedures are the same.

1. Disconnect the electrical connector from the washer pump.
2. Disconnect the hose from the washer pump.
3. Remove the washer pump from the washer solvent container.

### Installation Procedure

1. Install the washer pump in the washer solvent container.
2. Connect the hose to the washer pump.
3. Connect the electrical connector from the washer pump.