For 1990-2009 cars

#### 4T60-E COMPONENT LOCATION TABLE

Name | Location | Locator View (8A Cell 201 Figure #) | Connector End View (8A) | Group No.
--- | --- | --- | --- | ---
Automatic Transaxle | Lower LH side of engine compartment | 7 | -- | --
Automatic Transmission Shift Lock Control Actuator (BTSI) | Inside steering column near ignition switch | -- | -- | --
Backup Lamps | Part of taillamps | -- | -- | --
Body Control Module (BCM) | Below RH side of I/P, right of I/P compartment | 17 | 51-2 | --
Fuse Block | RH side of I/P, in RF door opening | -- | -- | --
Ignition Switch | Part of steering column | -- | -- | --
Instrument Cluster | LH side of I/P | 16 | 81-6 | --
LH Taillamp | Rear of vehicle, LH side | 42 | 202-43 | --
Powertrain Control Module (PCM) | Engine compartment, secured in air cleaner assembly | 12 | Engine Controls | --
RH Taillamp | Rear of vehicle, RH side | 42 | 202-51 | --
Rear Side Door Actuator Motor | RH quarter panel, above wheelhouse | 34 | 137-2 | --
Starter Solenoid | Lower front of engine, part of starter motor assembly | 7 | -- | --
Stop Lamp Switch | Mounted to brake pedal support | 19 | 202-53 | --
Transaxle Range Switch | Rear LH side of engine compartment, mounted to top of transaxle | 7 | 202-54 | --
Underhood (UH) Electrical Center | Engine compartment, front of RH wheelhouse, above battery | 1,8 | 202-55 | --
Vehicle Speed Sensor (VSS) | Lower RR of engine compartment, mounted to RH side of transaxle | 62 | -- | --
C103 (2 cavities) | I/P wiring harness to engine wiring harness, in lower LH side of engine compartment, next to C101 | 11 | 202-2 | --
C111 (7 cavities) | Engine wiring harness to automatic transaxle wiring harness, lower LH side of engine compartment, front of automatic transaxle | 7 | 202-4 | --
C200 (56 cavities) | I/P wiring harness to RH side of body wiring harness, behind RH side of I/P compartment, below P100 | 33 | 202-6 | --
C201 (48 cavities) | I/P wiring harness to steering column wiring harness, mounted to LH side of steering column near base | 15 | 202-9 | --
C203 (56 cavities) | I/P wiring harness to LH side of body wiring harness, LH side of steering column, below P101 | 33 | 202-12 | --
G113 | Engine compartment, left of starter, along with battery ground | 7 | -- | --
G401 | Secured to lower LH D-pillar | 59 | -- | --
P100 | On RH side of bulkhead, left of RH strut tower | 2 | -- | --
P101 | On LH side of bulkhead, right of LH strut tower | 11 | -- | --
P400 | Behind RH taillamp | 42 | -- | --
P401 | Behind LH taillamp | 42 | -- | --
S106 | Engine harness, front LH side of engine compartment approximately 10 cm (4 in) from powertrain control module (PCM) | -- | -- | --
S115 | Automatic transaxle harness, inside automatic transaxle housing approximately 42 cm (17 in) from automatic transaxle fluid temperature sensor | -- | -- | --
S122 | Engine harness, top LH side of radiator approximately 25 cm (10 in) from engine coolant fan #1 (RH) motor breakout | -- | -- | --
S209 | I/P harness, center of I/P approximately 8 cm (3 in) from security indicator lamp | -- | -- | --
S406 | Body harness, LR of body approximately 17 cm (7 in) from P401 breakout | -- | -- | --
S435 | Body harness, LR of body approximately 8 cm (3 in) from P401 | -- | -- | --