For 1990-2009 cars

### Removal Procedure

1. Remove the air filter element.
2. Disconnect the IAT sensor connector.
3. Disconnect the MAF sensor connector.
4. Remove the air inlet duct from the throttle body.
5. Remove the air cleaner housing cover.
6. Remove the air filter element.

### Installation Procedure

1. Install the air filter element.
2. Carefully align the air filter cover to the housing.
3. Install the air inlet duct to the throttle body.
4. Connect the MAF sensor connector.
5. Connect the IAT sensor connector.