For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door inner trim panel. Refer to Sliding Rear Side Door Trim Panel Replacement .
2. Remove the sliding door water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the sliding door latch screws (1,2 & 3).
4. When the sliding door latch is loose, unhook the latch/lock rod form the sliding door latch.
5. Remove the sliding door latch from the sliding door.

### Installation Procedure

1. Install the sliding door latch to the sliding door.
2. Hook the latch/lock rod to the sliding door latch.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the sliding door latch screws to the specified fastener tightening sequence.

Tighten
Tighten the screws to 10 N·m (89 lb in).

4. Install the sliding door water deflector. Refer to Rear Side Door Water Deflector Replacement .
5. Install the sliding door inner trim panel. Refer to Sliding Rear Side Door Trim Panel Replacement .