For 1990-2009 cars

### Removal Procedure

1. Press the video screen release button and flip the video screen to the down position.
2. Remove the two hinge cover screws.
3. Remove the hinge cover from the hinge.

### Installation Procedure

1. Install the hinge cover to the hinge.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the hinge cover screws.

Tighten
Tighten the hinge cover screws to 2 N·m (18 lb in).

3. Return the video screen to the up position.